---
title: "Connect a VX690 to a base station with Bluetooth"
url: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx690-user-manual/connect-a-vx690-to-a-base-station-with-bluetooth"
source_url: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx690-user-manual/connect-a-vx690-to-a-base-station-with-bluetooth.md"
canonical: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx690-user-manual/connect-a-vx690-to-a-base-station-with-bluetooth"
last_modified: "2019-04-19T08:44:00+02:00"
language: "en"
---

# Connect a VX690 to a base station with Bluetooth

[View source](/point-of-sale/user-manuals/terminal-deprecation/vx690-user-manual/connect-a-vx690-to-a-base-station-with-bluetooth.md)

Use a Bluetooth connection to pair the VX690 and the base station 

## Requirements

### Remove Wi-Fi profiles from the machine

1. Ensure the network is using DHCP.

2. Remove Wi-Fi profiles from the machine:

   1. Hold **![](/user/pages/reuse/image-library/buttons/07.confirmvx690/13_vx690.png)** + **9** to open the Admin menu. You may be prompted for a PIN.
   2. Pres&#x73;**&#xA0;1. Network**.
   3. Press **2. Wi-Fi**.
   4. Press **#** to scroll down.
   5. Press **4. Wi-Fi reset**.\
      The device will restart and Bluetooth can be switched to the default network.

3. Connect Bluetooth base to the power source using a mini USB cable.

4. Connect Bluetooth base to the network using the Ethernet connection (marked ETH on the base).

Once the terminal is paired to a Bluetooth base station, it should remain paired with it. If you have more than one terminal and base station, mark the base station and terminal to avoid mixing them up.

## Steps

1. Hold **![](/user/pages/reuse/image-library/buttons/07.confirmvx690/13_vx690.png)** +**&#xA0;9** to open the Admin menu. You may be prompted for a PIN.
2. Press **1.Network** **> 3.** **Bluetooth** **>** **2. Base Station** **>** **1. Scan**
3. Press the pairing button on the base station to make it discoverable. A blue light flashes on the base station.
4. Choose the base station from the list, and press **1. Pair.&#xA0;**&#x54;he base station will be listed with its serial number as its name.
5. Select the Bluetooth base serial number from the list of devices.
6. Press **3. Set Connection.**
7. Press **3. All\_Ports.**
8. Press the **![](/user/pages/docs/03.point-of-sale/48.user-manuals/26.terminal-deprecation/20.vx690-user-manual/05.connect-a-vx690-to-a-base-station-with-bluetooth/15_vx690.png)** button until you get back to the main Network menu and choose option **1. Connection Status**.
9. When connected successfully, the **Ethernet/BT** option should be set to **Connected**.
