---
title: "Charge the VX680"
url: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx680-user-manual/charge-the-vx680"
source_url: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx680-user-manual/charge-the-vx680.md"
canonical: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx680-user-manual/charge-the-vx680"
last_modified: "2019-04-18T18:08:00+02:00"
language: "en"
---

# Charge the VX680

[View source](/point-of-sale/user-manuals/terminal-deprecation/vx680-user-manual/charge-the-vx680.md)

Charge your terminal before use.

## Steps

1. Connect the charging cradle to the power supply cable, and then the power supply to the electrical grid.

2. Place the VX680 terminal on the cradle to charge the device and to power it on.

3. To fully charge the VX680, place it on the cradle for at least 6 hours, until the LED indicator remains lit.
