---
title: "Board the terminal - VX820"
url: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx820-user-manual/board-the-terminal-vx820"
source_url: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx820-user-manual/board-the-terminal-vx820.md"
canonical: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx820-user-manual/board-the-terminal-vx820"
last_modified: "2019-05-14T15:39:00+02:00"
language: "en"
---

# Board the terminal - VX820

[View source](/point-of-sale/user-manuals/terminal-deprecation/vx820-user-manual/board-the-terminal-vx820.md)

Board a terminal to register and use it with the Adyen payments platform.

## Requirements

* Board the terminal only after successfully connecting the device to the internet, and performing a device security inspection. For more information, see the [quick start guide](/point-of-sale/user-manuals/terminal-deprecation/vx820-user-manual).

## Steps

### Board with the Adyen App

1. Press **![](/user/pages/reuse/image-library/buttons/09.confirmvx820/15_vx820.png)** + **9** to open the admin menu.
2. Enter the PIN code for the Admin menu. If you do not know this code, see our [POS Troubleshooting section](/point-of-sale/pos-troubleshooting/terminal-turns-on/admin-pin/).\
   The terminal displays the Admin menu.
3. Press **1. Network**.
4. Press **2. Ethernet.**
5. Press **1**. **TCP/IP settings** to view and make a note of the terminal's IP address.
6. Download and install the Adyen POS App from the [Apple App Store](https://www.apple.com/app-store/) or the Google Play Store.

#### Board with an Android device

1. Open the Adyen POS App.
2. Enter the details of your API credentials. To learn how to retrieve these, see [Basic authentication](/development-resources/api-credentials#basic-authentication).
3. Tap **☰**.
4. Tap **Payment device**.\
   The app will prompt to select between Bluetooth and Wi-Fi connection.
5. Enter the IP address of your terminal and tap **Add Device**.\
   The Adyen POS App identifies the terminal, synchronizes with the Adyen payments platform, and verifies the terminal configuration.
6. The terminal begins boarding and restarts.\
   After rebooting, the terminal will begin to update to the latest merchant configuration. Once the latest configuration has been applied, you can begin processing payments.

#### Board with an iOS device

1. Open the Adyen POS App on the mobile device.
2. Tap the **![](/user/pages/reuse/image-library/buttons/13.bluetoothmenu/ic-pos-bluetooth-3x.png)**  icon.
3. Tap the '**+**' at the top of the **Payment device** popup menu.
4. Enter the device hostname or IP.\
   The device will now be listed in the **Payment device** menu with the status "Not Boarded".
5. Tap the name of the device.\
   The device shows a message saying the device is not configured, with options to **Cancel** or **Board device**.
6. Tap **Board Device**.
7. The terminal begins boarding and restarts.\
   After rebooting, the terminal will begin to update to the latest merchant configuration. Once the latest configuration has been applied, you can begin processing payments.

## Board the terminal with library integrations 

To board the terminal with your own custom systems, review our integration guides:

* [Java Native Interface Integration](/point-of-sale/classic-library-deprecation/classic-library-integrations/java-native-interface-integration)
* [COM Extension for Windows integration](/point-of-sale/classic-library-deprecation/classic-library-integrations/com-extension-for-windows-integration)
* [C Library Integration](/point-of-sale/classic-library-deprecation/classic-library-integrations/c-library-integration)
* [iOS Guide](/point-of-sale/classic-library-deprecation/classic-library-integrations/ios-integration)
* [Android guide](/point-of-sale/classic-library-deprecation/classic-library-integrations/android-integration).

If you have any issues boarding your terminal, see our [POS Troubleshooting](/docs/point-of-sale/pos-troubleshooting) section.
