---
title: "Turn on and turn off the VX675"
url: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx675-user-manual/turn-on-and-turn-off-the-vx675"
source_url: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx675-user-manual/turn-on-and-turn-off-the-vx675.md"
canonical: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx675-user-manual/turn-on-and-turn-off-the-vx675"
last_modified: "2019-04-18T16:57:00+02:00"
language: "en"
---

# Turn on and turn off the VX675

[View source](/point-of-sale/user-manuals/terminal-deprecation/vx675-user-manual/turn-on-and-turn-off-the-vx675.md)

Turn your terminal on to begin setting it up for payments.

## Turn on the VX675

* Hold **![](/user/pages/reuse/image-library/buttons/03.confirmvx675/6_vx675.png)** until the terminal displays the startup screen.

## Turn off the VX675

* Hold **![](/user/pages/docs/03.point-of-sale/48.user-manuals/26.terminal-deprecation/18.vx675-user-manual/02.turn-on-and-turn-off-the-vx675/7_vx675.png)**. The terminal will beep repeatedly and then turns off.
