---
title: "Install or replace paper rolls - VX690"
url: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx690-user-manual/install-or-replace-paper-rolls-vx690"
source_url: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx690-user-manual/install-or-replace-paper-rolls-vx690.md"
canonical: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx690-user-manual/install-or-replace-paper-rolls-vx690"
last_modified: "2019-04-19T08:45:00+02:00"
language: "en"
---

# Install or replace paper rolls - VX690

[View source](/point-of-sale/user-manuals/terminal-deprecation/vx690-user-manual/install-or-replace-paper-rolls-vx690.md)

Install paper rolls, or replace used rolls to print receipts.

***

The VX690 uses the following receipt paper:

* 57 mm x 40 mm x 12 mm thermal receipt paper

It is important you have sufficient stock of receipt paper, because without receipt paper it is not possible to accept payments.

## Steps

1. Gently pull the latch located on the top of the terminal to unlock the paper roll cover.
2. Lift the printer cover up and then back.
3. Remove any partial roll of paper in the printer tray by lifting it up.
4. Loosen the glued leading edge of the paper or remove the protective strip from the new roll of paper.
5. Unwind the paper roll past any glue residue.
6. Hold the roll so that the paper feeds from the bottom of the roll when the terminal is inverted.
7. Drop the paper roll into the printer tray.\
   ![](/user/pages/docs/03.point-of-sale/48.user-manuals/26.terminal-deprecation/20.vx690-user-manual/02.install-or-replace-paper-rolls-vx690/noText_vx690-Install-or-replace-paper-rolls.png)
8. Close the paper roll cover by gently pressing directly on the cover until it clicks shut. 
