---
title: "Get started manuals"
description: "Learn how to set up the terminal, connect it to your network, and use the menus."
url: "https://docs.adyen.com/point-of-sale/user-manuals"
source_url: "https://docs.adyen.com/point-of-sale/user-manuals.md"
canonical: "https://docs.adyen.com/point-of-sale/user-manuals"
last_modified: "2026-04-15T15:27:00+02:00"
language: "en"
---

# Get started manuals

Learn how to set up the terminal, connect it to your network, and use the menus.

Use this overview to see available payment terminals based on use case, location, and desired features.

If you do not need a physical terminal, look at our [mobile solutions](/point-of-sale/ipp-mobile). These enable you to accept Tap to Pay transactions on a mobile device like a smartphone, or using a combination of a mobile device and a card reader.

PCI PTS 5 payment terminals will no longer be available for order starting **April 30, 2026**.

## Available filters

Use case, Countries/Regions, Suitable for, Feature, Connectivity, PCI compliance

## Terminal catalog

### [AMS1 (Android)](/point-of-sale/user-manuals/ams1-user-manual)

Battery-powered Android payment terminal that you can turn into an all-in-one device by installing a POS app and other apps, like an inventory management app.

* **Use case**: Mobile
* **Countries/regions**: Australia (AU), Europe (EU), Hong Kong (HK), Japan (JP), Malaysia (MY), Mexico (MX), New Zealand (NZ), North America (NA), Singapore (SG), United Arab Emirates (UAE), United Kingdom (UK)
* **Connectivity**: Wi-Fi 2.4 Ghz, Wi-Fi 5 Ghz, Cellular 3G, Cellular 4G
* **Suitable for**: Integrated
* **Features**: Touchscreen, Power adapter, Replaceable battery, Camera
* **PCI compliance**: PCI PTS 6

### [e285p](/point-of-sale/user-manuals/e285-user-manual)

Pocket-sized terminal with a small display that you can connect to a tablet for on-the-go processing. Has a cellular connection fallback, but only up to 3G. The terminal runs on battery power and can be charged using a 5V DC, 1A charger (not included).

* **Use case**: Mobile
* **Countries/regions**: Australia (AU), Brazil (BR), Europe (EU), Hong Kong (HK), Malaysia (MY), Mexico (MX), New Zealand (NZ), North America (NA), Singapore (SG), United Arab Emirates (UAE), United Kingdom (UK)
* **Connectivity**: Wi-Fi 2.4 Ghz, Wi-Fi 5 Ghz, Cellular 3G, Bluetooth, Bluetooth PAN
* **Suitable for**: Integrated
* **Features**: Touchscreen, Replaceable battery, Physical PIN pad
* **PCI compliance**: PCI PTS 5

### [M400](/point-of-sale/user-manuals/m400-user-manual)

A terminal with a large display, ideal for showing line items like virtual receipts, and advertising. Or for collecting shopper input, such as a shopper's email address, signature, or survey feedback.

* **Use case**: Countertop
* **Countries/regions**: Australia (AU), Europe (EU), Hong Kong (HK), Malaysia (MY), Mexico (MX), New Zealand (NZ), North America (NA), Singapore (SG), United Arab Emirates (UAE), United Kingdom (UK)
* **Connectivity**: Wi-Fi 2.4 Ghz, Wi-Fi 5 Ghz, Ethernet
* **Suitable for**: Integrated
* **Features**: Touchscreen, Power adapter, Stylus pen, Physical PIN pad
* **PCI compliance**: PCI PTS 5

### [M450 (Android)](/point-of-sale/user-manuals/m450-user-manual)

Android terminal that is great for Impact, insights and two-way interactions. From branded logos and rich media advertising to input screens for loyalty program sign-up, surveys, and NPS.

* **Use case**: Countertop
* **Countries/regions**: Europe (EU), North America (NA), United Kingdom (UK)
* **Connectivity**: Wi-Fi 2.4 Ghz, Wi-Fi 5 Ghz, Ethernet
* **Suitable for**: Integrated
* **Features**: Touchscreen, Power adapter, Camera, Physical PIN pad
* **PCI compliance**: PCI PTS 6

### [P400 Plus](/point-of-sale/user-manuals/p400-plus-user-manual)

With its small footprint and Ethernet connection, the Verifone P400 Plus works well on a stationary retail counter.

* **Use case**: Countertop
* **Countries/regions**: Australia (AU), Brazil (BR), Europe (EU), Hong Kong (HK), Malaysia (MY), Mexico (MX), New Zealand (NZ), North America (NA), Singapore (SG), United Arab Emirates (UAE), United Kingdom (UK)
* **Connectivity**: Wi-Fi 2.4 Ghz, Wi-Fi 5 Ghz, Ethernet
* **Suitable for**: Integrated
* **Features**: Touchscreen, Power adapter, Physical PIN pad
* **PCI compliance**: PCI PTS 5

### [P630 (Android)](/point-of-sale/user-manuals/p630-user-manual)

With its premium design, Android operating system, and great feature and connectivity support, the Verifone P630 is a great choice for stationary retail counters.

* **Use case**: Countertop
* **Countries/regions**: Australia (AU), Europe (EU), Hong Kong (HK), Japan (JP), Malaysia (MY), New Zealand (NZ), North America (NA), Singapore (SG), United Arab Emirates (UAE), United Kingdom (UK)
* **Connectivity**: Wi-Fi 2.4 Ghz, Wi-Fi 5 Ghz, Ethernet
* **Suitable for**: Integrated
* **Features**: Touchscreen, Power adapter, Physical PIN pad
* **PCI compliance**: PCI PTS 6

### [S1E2L (Android)](/point-of-sale/user-manuals/s1e2l-user-manual)

A battery-powered Android payment terminal with a built-in barcode scanner. You can turn it into an all-in-one device by installing a POS app and other apps, like an inventory management app.

* **Use case**: Mobile
* **Countries/regions**: Australia (AU), Europe (EU), Hong Kong (HK), Japan (JP), Malaysia (MY), New Zealand (NZ), North America (NA), Singapore (SG), United Arab Emirates (UAE), United Kingdom (UK)
* **Connectivity**: Wi-Fi 2.4 Ghz, Wi-Fi 5 Ghz, Cellular 3G, Cellular 4G
* **Suitable for**: Integrated
* **Features**: Touchscreen, Power adapter, Replaceable battery, Camera, Barcode scanner, Fingerprint scanner
* **PCI compliance**: PCI PTS 6

### [S1E4Pro (Android)](/point-of-sale/user-manuals/s1e4pro-user-manual)

A battery-powered Android payment terminal that is drop-proof, dust-proof, splash-proof. NOTE: Currently not available in GER.

* **Use case**: Mobile
* **Countries/regions**: Australia (AU), Europe (EU), New Zealand (NZ), United Arab Emirates (UAE), United Kingdom (UK)
* **Connectivity**: Wi-Fi 2.4 Ghz, Wi-Fi 5 Ghz, Cellular 3G, Cellular 4G, Bluetooth
* **Suitable for**: Integrated
* **Features**: Touchscreen, Power adapter, Replaceable battery, Camera
* **PCI compliance**: PCI PTS 6

### [S1F2 (Android)](/point-of-sale/user-manuals/s1f2-user-manual)

A battery-powered Android payment terminal that you can turn into an all-in-one device by installing a POS app and other apps, like an inventory management app. Is has a camera, a built-in printer, and a barcode scanner.

* **Use case**: Mobile
* **Countries/regions**: Australia (AU), Brazil (BR), Europe (EU), Hong Kong (HK), Japan (JP), Malaysia (MY), Mexico (MX), New Zealand (NZ), North America (NA), Singapore (SG), United Arab Emirates (UAE), United Kingdom (UK)
* **Connectivity**: Wi-Fi 2.4 Ghz, Wi-Fi 5 Ghz, Cellular 3G, Cellular 4G
* **Suitable for**: Integrated, Standalone
* **Features**: Touchscreen, Power adapter, Replaceable battery, Camera, Barcode scanner, Printer
* **PCI compliance**: PCI PTS 6

### [S1F4Pro](/point-of-sale/user-manuals/s1f4pro-user-manual)

A battery-powered mobile terminal with Wi-Fi, Bluetooth, and 4G connectivity, a camera, and a built-in printer.

* **Use case**: Mobile
* **Countries/regions**: Australia (AU), Europe (EU), Malaysia (MY), North America (NA), United Kingdom (UK)
* **Connectivity**: Wi-Fi 5 Ghz, Cellular 3G, Cellular 4G, Bluetooth
* **Suitable for**: Integrated, Standalone
* **Features**: Touchscreen, Power adapter, Replaceable battery, Camera, Barcode scanner, Printer
* **PCI compliance**: PCI PTS 6

### [SFO1 (Android)](/point-of-sale/user-manuals/sfo1-user-manual)

Payment, branding, and customer engagement — all in one terminal.

* **Use case**: Countertop
* **Countries/regions**: Europe (EU), North America (NA)
* **Connectivity**: Wi-Fi 2.4 Ghz, Wi-Fi 5 Ghz, Cellular 4G, Ethernet
* **Suitable for**: Integrated
* **Features**: Touchscreen, Power adapter, Camera
* **PCI compliance**: PCI PTS 6

### [S1U2 (Android)](/point-of-sale/user-manuals/s1u2-user-manual)

An all-in-one Android payment terminal suitable for unattended environments and outdoor use. It has a front camera and a barcode scanner to support paying with a contactless card or a mobile wallet.

* **Use case**: Unattended
* **Countries/regions**: Australia (AU), Europe (EU), Hong Kong (HK), Japan (JP), Malaysia (MY), New Zealand (NZ), North America (NA), Singapore (SG), United Arab Emirates (UAE), United Kingdom (UK)
* **Connectivity**: Wi-Fi 2.4 Ghz, Wi-Fi 5 Ghz, Cellular 3G, Cellular 4G, Ethernet
* **Suitable for**: Integrated
* **Features**: Touchscreen, Camera, Barcode scanner
* **PCI compliance**: PCI PTS 6

### [UX300](/point-of-sale/user-manuals/ux300-user-manual)

The Verifone UX300 consists of the UX300 card reader, the UX100 PIN pad with a display, and the UX400 NFC-reader that allows shoppers to pay with a contactless card or a mobile wallet. These devices are intended for mounting in your self-service machine.

* **Use case**: Unattended
* **Countries/regions**: Australia (AU), Europe (EU), Hong Kong (HK), Malaysia (MY), New Zealand (NZ), North America (NA), Singapore (SG), United Arab Emirates (UAE), United Kingdom (UK)
* **Connectivity**: Ethernet
* **Suitable for**: Integrated
* **Features**: Power adapter, Physical PIN pad
* **PCI compliance**: PCI PTS 5

### [UX410](/point-of-sale/user-manuals/ux410-user-manual)

The Verifone UX410 terminals are no longer available for new orders. We recommend ordering S1U2 terminals. The Verifone UX410 is an NFC-reader that allows shoppers to pay with a contactless card or a mobile wallet. It is ideal as a standalone payment device for quick, low-value transactions in a self-service environment.

* **Use case**: Unattended
* **Connectivity**: Ethernet
* **Suitable for**: Integrated
* **Features**: Power adapter
* **PCI compliance**: PCI PTS 5

### [V240m Plus](/point-of-sale/user-manuals/v240m-user-manual/)

Only available in Brazil. Can be powered by a power adapter, or with the included battery pack. It has a built-in printer for mobile transaction processing, and 3G fallback. The SIM card is multi-carrier, so you can select the best 3G provider in the region.

* **Use case**: Mobile
* **Countries/regions**: Brazil (BR)
* **Connectivity**: Wi-Fi 2.4 Ghz, Wi-Fi 5 Ghz, Cellular 3G, Bluetooth
* **Suitable for**: Integrated, Standalone
* **Features**: Touchscreen, Power adapter, Replaceable battery, Printer, Physical PIN pad
* **PCI compliance**: PCI PTS 5

### [V400c Plus](/point-of-sale/user-manuals/v400c-user-manual)

Similar to the P400, the Verifone V400c Plus works well on a stationary retail counter. It offers a small footprint, an Ethernet connection, and a built-in printer.

* **Use case**: Countertop
* **Countries/regions**: Australia (AU), Europe (EU), Hong Kong (HK), Japan (JP), Malaysia (MY), Mexico (MX), New Zealand (NZ), North America (NA), Singapore (SG), United Arab Emirates (UAE), United Kingdom (UK)
* **Connectivity**: Wi-Fi 2.4 Ghz, Wi-Fi 5 Ghz, Ethernet
* **Suitable for**: Integrated, Standalone
* **Features**: Touchscreen, Power adapter, Printer
* **PCI compliance**: PCI PTS 5

### [V400m](/point-of-sale/user-manuals/v400m-user-manual)

Can be powered by a power adapter, or with the included battery pack. It has a built-in printer for mobile transaction processing, and 4G fallback.

* **Use case**: Mobile
* **Countries/regions**: Australia (AU), Europe (EU), Hong Kong (HK), Japan (JP), Malaysia (MY), Mexico (MX), New Zealand (NZ), North America (NA), Singapore (SG), United Arab Emirates (UAE), United Kingdom (UK)
* **Connectivity**: Wi-Fi 2.4 Ghz, Wi-Fi 5 Ghz, Cellular 3G, Cellular 4G, Bluetooth
* **Suitable for**: Integrated, Standalone
* **Features**: Touchscreen, Power adapter, Replaceable battery, Printer, Physical PIN pad
* **PCI compliance**: PCI PTS 5

### [V400m with base station](/point-of-sale/user-manuals/v400m-with-bt-base)

Using the Bluetooth base station, you can power the terminal and connect the terminal to your Ethernet LAN. The terminal has a built-in printer for mobile transaction processing, and 4G fallback.

* **Use case**: Mobile
* **Countries/regions**: Australia (AU), Europe (EU), Hong Kong (HK), Japan (JP), Malaysia (MY), Mexico (MX), New Zealand (NZ), North America (NA), Singapore (SG), United Arab Emirates (UAE), United Kingdom (UK)
* **Connectivity**: Wi-Fi 2.4 Ghz, Wi-Fi 5 Ghz, Cellular 3G, Cellular 4G, Ethernet, Bluetooth
* **Suitable for**: Integrated, Standalone
* **Features**: Touchscreen, Power adapter, Replaceable battery, Printer, Physical PIN pad, Base station
* **PCI compliance**: PCI PTS 5
