---
title: "Turn on and turn off the VX680"
url: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx680-user-manual/turn-on-and-turn-off-the-vx680"
source_url: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx680-user-manual/turn-on-and-turn-off-the-vx680.md"
canonical: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/vx680-user-manual/turn-on-and-turn-off-the-vx680"
last_modified: "2019-04-18T18:07:00+02:00"
language: "en"
---

# Turn on and turn off the VX680

[View source](/point-of-sale/user-manuals/terminal-deprecation/vx680-user-manual/turn-on-and-turn-off-the-vx680.md)

Turn your terminal on to begin setting it up for payments.

## Turn on the VX680

1. Press and hold **![](/user/pages/reuse/image-library/buttons/05.confirmvx680/9_vx680.png)** for a couple of seconds.
2. When the terminal is fully booted, it displays the Adyen logo or your custom logo, in case you provided us with a logo and we have already registered the terminal to your account.

## Turn off the VX680

* Press and hold **![](/user/pages/docs/03.point-of-sale/48.user-manuals/26.terminal-deprecation/19.vx680-user-manual/03.turn-on-and-turn-off-the-vx680/10_vx680.png)**. The terminal will beep repeatedly and then power down.
