---
title: "Remove the e355 from the frame"
description: "Remove the terminal from the frame when it is no longer in use."
url: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/e355-user-manual/attach-and-use-the-e355-frame/remove-the-e355-from-the-frame"
source_url: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/e355-user-manual/attach-and-use-the-e355-frame/remove-the-e355-from-the-frame.md"
canonical: "https://docs.adyen.com/point-of-sale/user-manuals/terminal-deprecation/e355-user-manual/attach-and-use-the-e355-frame/remove-the-e355-from-the-frame"
last_modified: "2019-04-23T17:38:00+02:00"
language: "en"
---

# Remove the e355 from the frame

Remove the terminal from the frame when it is no longer in use.

[View source](/point-of-sale/user-manuals/terminal-deprecation/e355-user-manual/attach-and-use-the-e355-frame/remove-the-e355-from-the-frame.md)

## Steps

1. Unlock the frame by turning the locking screws counter-clockwise.

2. Push the Eject button downwards to release the e355 from the frame.

3. Turn the locking screws clockwise.

When attaching or removing the tablet, place the e355 on a smooth flat surface, to avoid scratching the tablet screen.
